

**Figure S5.** Growth curve at laboratory scale of *B. megaterium* LVN01 in Biogas digestate, operational conditions: 10 mL, 200 rpm, 30.8 °C, pH 7.0.