Figure 1: Classification of the NGDO according to their efficiency